Instructions for Jms539b multi-bay firmware updating


**Notes:**

To make sure the products work better with HD player or Linux.


Applicable models:（3549SUSJ3，3559SUSJ3，3549RUS3，3559RUS3，9548U3, 9548RU3, 9558U3, 9558RU3）

**How to update:**


1．Unzip the firmware file




2. Run the FwUpdateTool\_v1\_16\_12





3．Run the updating file in Windows XP, you can see the status of the product:



4.Check the current chip version （JMS539）and FW version（31.00.40.06）



5.Click  to load .bin file，Click  to update.



6，Power off and re-power on to check the FW version, if it shows: version 00.00.40.16, the updating is finished successfully.

